F0 00 00 50 29 00 F7
{ Clear All Settings - allow all MIDI events not specified below to pass through unchanged }

F0 00 00 50 29 02 00 00 02 00 7F 01 03 01 7F 03 03 01 7F F7
97 00 00
B7 29 00
{ Setting #1: Map all Note-On events of velocities 1 - 127 on MIDI channel 8 to Control Change #41 events on MIDI channel 8, with the incoming velocity mapped to the outgoing Control Change value. Continue to process settings  (right-click to edit) }

F0 00 00 50 29 02 01 00 02 00 7F 01 03 00 7F 02 02 00 7F 03 03 00 7F F7
97 00 00
97 00 00
{ Setting #2: Map all Note-On events on MIDI channel 8 to Note-On events on MIDI channel 8, with the incoming Note number mapped to the outgoing Note number, and the incoming velocity mapped to the outgoing velocity value. Continue to process settings  (right-click to edit) }